20 mm

20 mm – Turning-in Edge width

**A** = Double (2x) Turning-in Edge width - (minus) 6 or 7 or 8mm

Cardboards from 1,00 to 1,40 mm thick [**A** – (minus) 6mm = **B** = 4mm]

Cardboards from 1,50 to 1,90 mm thick [**A** – (minus) 7mm = **B** = 5mm]

Cardboards from 2,00 to 2,5 mm thick [**A** – (minus) 8mm = **B** = 6mm]

**Exemple: Cardboard 1,7mm thick and 20mm Turning-in Edge**

Turning-in doubled width 40mm

**A** = 34 – 7mm = **28mm**

**B** = 5mm after cutting

**B**

**B**

**A**

**A**

20 mm

20 mm

**Tünkers Pneumatic Corner Cutter CTA 30**

Cutting adjustment for straight cut.

Straight and round corner are standards but special cuts are also possible due to its blade mounted in wooden board.

Bookbinding; finishing equipment; pneumatic cutting; hardcoverbooks

Canteadeira Pneumática CTA 30 Tünkers

Ajuste de corte reto.

Cortes retos e redondos são padrão mas devido às lâminas cravadas em madeira como no corte e vinco, é possível realizar cortes especiais.